|  |
| --- |
| 12.jpg |

**Product Overview:**

PWM air cooling solution equipped with high efficiency fins and compact profile; works with most current Intel motherboard designs. **Only for Intel chipset configurations.**

**Specifications**

|  |  |
| --- | --- |
| Model  | Verkho i |
| Base Material | Aluminum |
| Dimension | 103 x 103 x 45mm |
| TDP(Thermal Design Power) | 90 |
| Fan | Speed | 1200-2500 rpm  |
| Connector | PWM 4-Pin |
| Dimension | 80 x 80 x 25mm |
| Bearing Type | Hydraulic Bearing |
| Started Voltage | 6V |
| Rated Voltage | 12V |
| Rated Current | 0.19 A  |
| Power Consumption | 2.28 Watts (One Fan) |
| Air Pressure | 0.53-1.21 mm-H2O |
| Air Flow | 25.15-58.25 CFM |
| Noise | 12.2-29.7dBA |
| MTBF(Mean Time Before Failure) | 60000 hrs. |
| Socket | LGA 1150/1151/1155/1156/775 |

**Warranty**

1 year

**Features**

* TDP (Thermal Design Power) up to 90W.
* Upgraded high efficiency fins for optimal thermal performance.
* Compact profile capable of mounting single 80mm fan configurations; works with most current Intel motherboard designs. **Only for Intel chipset configurations.**

**Package Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Name** | **Product Number** | **EAN CODE** | **UPC CODE** |
| Verkho i | ACTC-NA10010.01 | 4710700950791 |  |
|  |  |  |  |
| **Carton Size ( L x W x H )** | 540 x 335 x 235 mm | **Carton Weight**  | N.W 11.5 kg / G.W 12.8 kg |
| **Retail Box Size ( L x W x H )** | 105 x 105 x 55 mm | **Retail Box Weight**  | N.W 152 g / G.W 192 g |
| **Carton Qty** | 60 pcs | **Pallet Qty** | 3240(GP)/3600(HQ) |