|  |
| --- |
| 2.jpg |

**Product Overview:**

Comes with 2 ultra-efficient thermal heat pipes. Capable of mounting single 120mm fan configurations. PWM air cooling solution powered by Heat Core Touch Technology (HCTT) and equipped with high efficiency fins. Compatible with most current motherboard designs.

**Specifications**

|  |  |  |
| --- | --- | --- |
| Model | | Verkho 2 Plus |
| Base Material | | Aluminum block with HCTT Heat Core Touch Technology |
| Fin Material | | Aluminum |
| Heat pipe | | 6mm x 2 |
| Dimension | | 125 x 72 x 140mm |
| TDP(Thermal Design Power) | | 115 |
| Fan | Speed | 1000-2000 rpm |
| Connector | PWM 4-Pin |
| Dimension | 120 x 120 x 25mm |
| Bearing Type | Hydraulic Bearing |
| Started Voltage | 5V |
| Rated Voltage | 12V |
| Rated Current | 0.2 A |
| Power Consumption | 2.4 Watts |
| Air Pressure | 0.78-1.24 mm-H2O |
| Air Flow | 29.1-55.6 CFM |
| Noise | 18.2-26.7 dBA |
| MTBF  (Mean Time Before Failure) | 60000 hrs. |
| Socket | | LGA 1156/1155/1151/1150/775 AM4/AM3+/AM3/AM2+/AM2/FM2/FM1 |

**Warranty**

1 year

**Features**

* TDP (Thermal Design Power) up to 115W.
* Compact side flow air cooler for maximum compatibility.
* Heat Core Touch Technology and 2 ultra-efficient thermal heat pipes.
* Upgraded high efficiency fins for optimal thermal performance.
* Ultra-slim profile capable of mounting single 120mm fan configurations; works with most current motherboard designs.

**Package Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Name** | **Product Number** | **EAN CODE** | **UPC CODE** |
| Verkho 2 Plus |  |  |  |
|  |  |  |  |
| **Carton Size ( L x W x H )** | 425 x 330 x 365 mm | **Carton Weight** |  |
| **Retail Box Size ( L x W x H )** | 135 x 104 x 175 mm | **Retail Box Weight** |  |
| **Carton Qty** | 18 pcs | **Pallet Qty** |  |