|  |
| --- |
| C:\Users\Sky\Pictures\Tony_RU\AirCooling_03.jpg |

**Product Overview:**

Capable of mounting single 120mm fan configurations. PWM air cooling solution equipped with high efficiency fins and compact profile. Compatible with most current motherboard designs. **Not compatible with Intel 2011 and 2066.**

**Specifications**

|  |  |
| --- | --- |
| Model  | Verkho Plus |
| Base Material | Aluminum |
| Dimension | 128 x 128 x 68mm |
| TDP(Thermal Design Power) | 110 |
| Fan | Speed | 1000-2000 rpm  |
| Connector | PWM 4-Pin |
| Dimension | 120 x 120 x 25mm |
| Bearing Type | Hydraulic Bearing |
| Started Voltage | 6V |
| Rated Voltage | 12V |
| Rated Current | 0.25 A  |
| Power Consumption | 3.0 Watts |
| Air Pressure | 0.48-1.19 mm-H2O |
| Air Flow | 29.45-57.23 CFM |
| Noise | 10.4-26.5dBA |
| MTBF(Mean Time Before Failure) | 60000 hrs. |
| Socket | LGA 1156/1155/1151/1150/775 AM4/AM3+/AM3/AM2+/AM2/FM2/FM1 |

**Warranty**

1 year

**Features**

* TDP (Thermal Design Power) up to 110W.
* Upgraded high efficiency fins for maximum thermal performance.
* Compact profile capable of mounting single 120mm fan configurations; works with most current AMD and Intel motherboard designs. **Not compatible with Intel 2011 and 2066.**

**Package Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Name** | **Product Number** | **EAN CODE** | **UPC CODE** |
| Verkho Plus | ACTC-NA30020.01 | 4710700950814 |  |
|  |  |  |  |
| **Carton Size ( L x W x H )** | 535 x 405 x 394 mm | **Carton Weight**  | N.W 15.4 kg / G.W 16.6 kg |
| **Retail Box Size ( L x W x H )** | 130 x 130 x 88 mm | **Retail Box Weight**  | N.W 172 g / G.W 320 g |
| **Carton Qty** | 48 pcs | **Pallet Qty** | 960(GP)/1152 (HQ) |